

|  |
| --- |
| **OFFICIAL [PARTNERS]** |
| NOTIFICATION OF MOVEMENT OF ABNORMAL LOADS |
|  |
| Form of Notice to Police for Movement of Abnormal Indivisible Loads under Construction and Use Regulations (Northern Ireland) 1999 (subject to prior agreement of each Police Force to which this Notice is sent, it may be used to give Notice of Additional Journeys, Different Vehicles, Routes and Destinations). |
|  |
| List Police Forces to which this Form is sent: |  | Operator |       |
|       |  | Address |       |
|       |  |  |       |
|       |  | Telephone/Fax |       |
|       |  | Operator’s Licence No |       |
|       |  | Operator’s Reference No |       |
|  |  |  |  |
| The route and Department of Environment (Roads Service) (NI) Reference Number (if applicable) proposed to be used is |
| Particulars of Journey | **From (Full Address)** | **Date/Time** |  | Route/Reference No *(if applicable)* |
|  |       |       |  |       |
|  |  |        |  |  |
|  |  |  |  |  |
|  | **To (Full Address)** | **Date/Time** |  |  |
|  |       |       |  |  |
|  |  |        |  |  |
|  |  |  |
| Particulars of Vehicle | **Registration No****of Vehicle** | **Type of****Vehicle** | **Description of****Load** |  |  |
|  |       |       |       |  |  |
|  |  |
|  | OverallLength ofVehicle |       | Projection- Front |       | Projection- Rear |       | TotalLength |       |
|  |  |
|  | Overall Width |       | \*Maximum Height |       | Gross Weight orGross Train Weight |       |
|  | \*Loads in excess of 4.88 metres high must be informed to DOE (Roads Service) |
|  | All Axle Weights and Spacings with C & U Limits |

|  |
| --- |
| We hereby agree |
|  | Owner/Agent’s Signature |       | Date |       |
|  |
| Applicable to Northern Ireland | (a) | The marking of Projecting Loads and Fixed Appliances or Apparatus which Project should be marked in accordance with Schedule 15 of the Motor Vehicles (Construction and Use) Regulations (Northern Ireland) 1999. |
|  |  |
| (b) | Where the vehicle or load has an overall width exceeding 3.5 metres or where the overall length of a vehicle or of the vehicle together with any forward or rearward projection of its load exceeds 18.65 metres then an attendant is required. |
|  |  |
| (c) | Where the vehicle or load has an overall width exceeding 3.66 metres but not exceeding 4.3 metres an escort vehicle must be provided by the haulier. |
|  |
|  | **Note:** | Legislation on the Movement of Abnormal Loads under Construction and Use can be found in Regulation 79 and Schedule 15 of the Motor Vehicles (Construction and Use) Regulations (Northern Ireland) 1999. |
|  |
| Send completed forms to arrive at least 2 working days before proposed movement to: |
|  |
| **Police Service of Northern Ireland, Traffic Urban Region, Abnormal Loads Office, Police Sprucefield,** **4-8 Ravarnet Road, Lisburn BT28 5NB. Telephone Number (Direct) 028 9258 9126 or 101 Ext 67126.****Fax 028 9090 1251.** |
|  |
| *THIS FORM MAY ALSO BE USED TO NOTIFY OTHER POLICE FORCES* |